## Attachment G - Example of a Sample Flush Tag

FLUSH TAG

**Water outlet sampling in progress. Please do not use water**

School District Name: \_ (**INSERT SCHOOL DISTRICT NAME)** Date Flushed:

School Name: Flushing Process

School Address: Start Time:

Location of flushed outlet: End Time:

Is the fountain front cover removed for the sampler to determine the reservoir type (circle one): YES / NO

Person responsible for the flushing process (print name): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\* Water within the school distribution system should sit in the pipes unused for at least eight (8) hours after flushing but not more than 48 hours before a sample is taken.\*

*Note to the person responsible for the flushing process:*

A. Turn-off lawn sprinkler outlet(s) until water sampling is complete.

B. Make sure sampling outlets are accessible.