STRUCTURAL EVALUATION

CONSULTANT NAME	RATING PERIOD
PROJECT ENGINEER	DATE
STRUCTURE NO.

BRIDGE CHECK LIST

DOCUMENTED ERRORS REPORT	YES
Summary
1. Structural Data Included?
2. “Work Done” Section Included?
3. Rating Summary Provided?
Conclusions & Recommendations
4. Are Conclusions provided?
5. If bridge is Structurally Deficient or Functionally Obsolete, is major work recommended?
6. Are Priority 2 Repairs property identified and letters written in accordance with procedures?
7. Is load rating analysis provided and correct (if calculated this cycle)? Updated where necessary (or recommended for update)?
8. Is loss of section considered where appropriate?
9. Is controlling member identified?
10. Are allowable stresses given?
11. Are cadd drawings provided as per scope of work?

Sounding profiles done in accordance with underwater inspection manual?

Vertical and Lateral underclearance sketch?
12. Are field notes complete with proper field note sheets present (i.e.-Fatigue Details, Substructure Scour, Waterway and Underclearance Sketches)?
Structural Inventory and Appraisal Sheets
13. Is SI & A Sheet #1 & #2 (or A, B, C, etc.) included and filled out?
14. Are Items 92 & 93 updated with the submission of the Item 90 inspection date?
15. Are condition ratings consistent with the report?
16. Are Items 41, 51, 53, 54, 55, 56 of the SI & A consistent with the field conditions?
17. Are Items 26 & 104 of the SI & A correct?
18. Is Item 106 of the SI & A correct?
19. Is Item 100 (Strahnet) coded correctly?
20. Are Items 112 & CP of the SI & A correct?
Pontis
21. Is the Pontis sheet included and complete with proper elements and fewer than 3 errors?
Field Verification Review

Dialogue with Consultant Project manager must occur prior to final determination due to possibility defects occurred subsequent to inspection
22. Major area of deterioration (large spalls, severe scaling, wide concrete cracks, steel fatigue cracks, collision damage, etc.) not documented or mis-documented in report.

STRUCTURAL EVALUATION

njdot

2004-09-23

TPSPALM

njdot